set background

Premise: controller adopts websocket to communicating once enter the platform system

Server sending data

{

"type":"place\_group\_ad",

"task":{

"id":"5e673567908de9e019fbf230",

"media\_id":"5e802fad8ef9d7a431ed9b14",

"task\_id":"5e89bdf18283968413a4503e",

"background\_type":"" //background type

}

}

//background\_type support types in below

"route", //route

"brake", //brake

"turn\_left",//turn left

"turn\_right",//turn right

"vacant", //vacant

"hired",//hired

"no\_service", //no service

"booked", //booked

"logo", //logo

​

Device return data

{

"type":"set\_taxi\_background", //

"task\_id":"5e89bdf18283968413a4503e",

"id":"5e673567908de9e019fbf230"

}

​

Switch link address

premise：controller adopts websocket to communicating once enter the platform system

Server sending data

​

{

"type":"switch\_taxi\_account",

"task":{

"id":"5e673567908de9e019fbf230",

"task\_id":"5e89bdf18283968413a4503e",

"account\_id\_token":"xxxx", //issued token

"taxiServerURL":"http://xxxx", //server address

"taxiServerTLSURL":"https://xxxx" //server address

}

}

Device return data

{

"type":"switch\_taxi\_account",

"id":"5e673567908de9e019fbf230",

"task\_id":"5e89bdf18283968413a4503e",

}

The server sending command of disconnecting device after receiving the return data from the device

{

"type":"time\_to\_disconnect",

"task":{

"id":"5e673567908de9e019fbf230",

"task\_id":"5e89bdf18283968413a4503e",

"account\_id\_token":"xxxx",

"taxiServerURL":"http://xxxx"

}

}

Query ads sort

premise：controller adopts websocket to communicating once enter the platform system

Server sending data

{

"type":"get\_advertise\_order",

"task":{

"id":"xxxxxx",

"task\_id":"xxxxxxx"

}

}

Device return data

{

"type":"get\_advertise\_order",

"task\_id":"5e89bdf18283968413a4503e",

"id":"5e673567908de9e019fbf230",

"advertise\_order":["xxxxx","xxxxx","xxxxxx"] //string type array, it is each item is ads

}

Query device ads

premise：controller adopts websocket to communicating once enter the platform system

Server sending data

{

"type":"get\_ad\_list",

"task":{

"id":"xxxxxx",

"task\_id":"xxxxxxx"

}

}

Device return data

​

{

"type":"get\_ad\_list",

"task\_id":"5e89bdf18283968413a4503e",

"id":"5e673567908de9e019fbf230",

"ad\_list": ["5e673567908de9e019fbf230","5e673567908de9e019fbf230"],//all ads list content

"current\_play\_list":["5e673567908de9e019fbf230"]

//List of currently playing advertising content

}

Switch of report play log

premise：controller adopts websocket to communicating once enter the platform system

Json data format

// switch of report play log

{

"type":"update\_player\_log\_switch",

"task":{

"id":"5e89bdf18283968413a4503e",

"task\_id":"5e89bdf18283968413a4503e",

"turn\_on":true //true open false close }

}

​

//return data

{

"type":"update\_player\_log\_switch",

"task\_id":"5e89bdf18283968413a4503e",

"id":"5e89bdf18283968413a4503e"

}

​

​

// switch of report GPS log

{

"type":"update\_gps\_log\_switch",

"task":{

"id":"5e89bdf18283968413a4503e",

"task\_id":"5e89bdf18283968413a4503e",

"turn\_on":true //true open false close

}

}

​

//return data

{

"type":"update\_gps\_log\_switch",

"task\_id":"5e89bdf18283968413a4503e",

"id":"5e89bdf18283968413a4503e"

}

​